Project Opensky 747V4
Version905 Update. (SP3)


This file is a full service pack from the 747V4series.
Advanced Animation kit (747V4Advanced) is already included.


Changes at 905 SP3
1.Added Towing car
2.New Posky Utility
3.Now cargo goes out (Use Posky Utility)

Changes at 720 SP1
1.Wing is smoothen at edge
2.Flap guide cover extention timing has been fixed.
3.Body gear steerling is now linked from nose gear.
4.Removed the roof of the beltloader for installing the stair car to the 747-200F

Am I using a 747V4Adv model?
=============================================
Please see the models gear when landing.
If the main gear (body gear) sinks in to the ground , then it's not a Advanced model.


How to install: 
1.For users who are using the 747V4Adv models 
===============================================
For the user who is already using the Advanced set (Posky747V4A) 
Just copy the Model file to the Model folder and texture to the texture (If exists )folder of the aircraft.
Then it should work.

2.For the users who doesn't use a Advanced model
==================================================
1.Copy the mdl file to the existing Project Opensky 747V4s folder.
2.Copy the "Posky744" folder inside the panel folder to the panel folder.
3.Add line under to your panel.cfg
[VCockpitXX] 's XX under depends on panel you use.
If using default FS2004 747-400 , should be [VCockpit03]
And before the [color] section.

If inside panel.cfg is only alias=
Then first copy the default 747-400's panel folder and do from 2.


Posky747V4Advanced
Created by Hiroshi Igami
Supported by Edward Cox 


============================================================================================

[VCockpitXX]
size_mm=512,512
pixel_size=512,512
texture=$Posky_ACU
background_color=0,0,0
gauge00=Posky744!PkyCALC, 140,80,140,80
gauge01=Posky744!PkyNosegearheight, 140,80,140,80
gauge02=Posky744!PkyBodygearheight, 140,80,140,80
gauge03=Posky744!PkyWinggearheight, 140,80,140,80
gauge04=Posky744!PkyLeftgearboggie, 140,80,140,80
gauge05=Posky744!PkyRightgearboggie, 140,80,140,80
gauge06=Posky744!PkyLeftwgearboggie, 140,80,140,80
gauge07=Posky744!PkyRightwgearboggie, 140,80,140,80
gauge08=Posky744!PkyNosegearsteerling, 140,80,140,80
gauge09=Posky744!PkyWINGROOTFLEX, 140,80,140,80
gauge10=Posky744!PkyRWINGMIDFLEX, 140,80,140,80
gauge11=Posky744!PkyRWINGTIPFLEX, 140,80,140,80
gauge12=Posky744!PkyLWINGMIDFLEX, 140,80,140,80
gauge13=Posky744!PkyLWINGTIPFLEX, 140,80,140,80
gauge14=Posky744!PkyRudder, 140,80,140,80
gauge15=Posky744!Pky_PB_Towhead, 140,80,140,80
