EMBRAER EMB-110 BANDEIRANTE

REFERENCE INFORMATION
For Standard procedures, see the Checklists tab.

Max. total aircraft weight take-off | 12,489 lbs
Max. total aircraft weight landing | 12,000 lbs

NOTE: To adjust fuel and payload, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 263 KIAS
MMO - Maximum Operating Speed Mach | .58 Mach
Turbulent Air Penetration Speed | 160 KIAS
VLE - Maximum Gear Operating Speed | 180 KIAS
VLO - Maximum Gear Retraction Speed | 180 KIAS
VA - Maneuvering Speed | 165 KIAS
VMC - Minimum Control Speed | 94 KIAS
VX - Two-engine Best Angle-of-Climb | 125 KIAS
VY - Two-engine Best Rate of Climb | 140 KIAS
Best Glide Speed both engines inoperative | 135 KIAS
Recommended Speed in Waiting Procedure | 140 KIAS

Maximum Flap Placard Speeds

Flaps | KIAS
25% | 200
50% | 160
75% | 140
100% | 125

V1 - Takeoff Decision Speed dry runway; flaps up
Standard temperature, 5,000' pressure altitude

12,489 lbs | 108 KIAS
<10,000 lbs | 104 KIAS

VR - Rotation Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

12,489 lbs | 111 KIAS
<10,500 lbs | 104 KIAS

V2 - Takeoff Safety Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

12,489 lbs | 117 KIAS
<10,500 lbs | 111 KIAS

Cruise Climb

Sea level to 10,000 | 160 KIAS
10,000 to 15,000 | 155 KIAS
15,000 to 20,000 | 150 KIAS

VREF - Landing Approach Speed flaps down; gear down

12,489 lbs | 110 KIAS
11,000 lbs | 105 KIAS
10,000 lbs | 102 KIAS
<10,000 lbs | 100 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.