BEECHCRAFT C99
REFERENCE INFORMATION
For standard procedures, see the Checklists tab.

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 243 KIAS
MMO - Maximum Operating Speed Mach | .50 Mach
Turbulent Air Penetration Speed | 170 KIAS
VLE - Maximum Gear Operating Speed | 184 KIAS
VLO - Maximum Gear Retraction Speed | 166 KIAS
VA - Maneuvering Speed | 184 KIAS
VMC - Minimum Control Speed | 94 KIAS
VX - Two-engine Best Angle-of-Climb | 125 KIAS
VY - Two-engine Best Rate of Climb | 140 KIAS
Best Glide Speed both engines inoperative | 135 KIAS

Maximum Flap Placard Speeds

Flaps | KIAS
Approach | 202
Full extension | 158

V1 - Takeoff Decision Speed dry runway; flaps up
Standard temperature, 5,000' pressure altitude

15,000 lbs | 108 KIAS
<10,500 lbs | 104 KIAS

VR - Rotation Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

15,000 lbs | 111 KIAS
<10,500 lbs | 104 KIAS

V2 - Takeoff Safety Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

15,000 lbs | 117 KIAS
<10,500 lbs | 111 KIAS

Cruise Climb

Sea level to 10,000 | 170 KIAS

VREF - Landing Approach Speed flaps down; gear down

15,000 lbs | 109 KIAS
14,000 lbs | 105 KIAS
13,000 lbs | 102 KIAS
12,000 lbs | 100 KIAS
11,000 lbs | 100 KIAS
10,000 lbs | 100 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.