BEECHCRAFT C99 PROCEDURES
For suggested speeds, see the Reference page of the Kneeboard.
Note that most actions can also be performed using the mouse.

BEFORE ENGINE STARTING |
[ ] Parking Brake | SET (press CTRL+PERIOD key)
[ ] Landing Gear Control | CHECK DOWN
[ ] Power Levers | IDLE (press F2 until Idle)
[ ] Propeller Controls | FULL FORWARD (press CTRL+F3 until fully in)
[ ] Condition Levers | FUEL CUTOFF (press CTRL+SHIFT+F2 until fully out)
[ ] Fuel Quantity | CHECK
[ ] Anti-ice | ON
[ ] Beacon | ON
ENGINE STARTING (BATTERY) |
Press CTRL+E to initiate engine autostart sequence, or:
[ ] Battery Switch | ON
[ ] Beacon | ON
[ ] Propeller Area | CLEAR
[ ] Fuel Flow | ON (press CTRL+SHIFT+F4)
[ ] Right Ignition and Engine Start Switch | ON (click and hold until engine starts)
[ ] Right Condition Lever | LOW IDLE (after the N1 Turbine RPM has stabilized, 12% minimum)
[ ] Right ITT and N1 Turbine RPM | MONITOR
[ ] Right Condition Lever | HIGH IDLE
[ ] Right Generator | ON
[ ] Left Ignition and Engine Start Switch | ON (Click and hold until engine starts)
[ ] Left Condition Lever | LOW IDLE (after the N1 Turbine RPM has stabilized, 12% minimum)
[ ] Left ITT and N1 Turbine RPM | MONITOR
[ ] Left Condition Lever | HIGH IDLE
[ ] Right Condition Lever | REDUCE TO LOW IDLE
[ ] Left Generator | ON
[ ] Avionics Master Switch | ON
BEFORE TAKEOFF (RUNUP) |
[ ] Avionics | CHECK
[ ] Autopilot | CHECK
| CHECK
[ ] Trim Tabs | SET (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Primary Governors | EXERCISE AT 1500 RPM
[ ] Manual Propeller Feathering | CHECK
[ ] Anti-ice | AS REQUIRED
[ ] Fuel Quantity, Flight, and Engine Instruments | CHECK
BEFORE TAKEOFF (FINAL ITEMS)
[ ] Annunciator Lights | EXTINGUISHED OR CONSIDERED
[ ] Transponder | ON ALT
[ ] Lights | AS REQUIRED
[ ] Anti-ice | AS REQUIRED
[ ] Takeoff speeds (V1, VR, and V2) | CONFIRM
TAKEOFF |
[ ] Brakes | HOLD
[ ] Power Levers | 100% N1 TURBINE RPM (OBSERVE ITT LIMITS) (press F3 as necessary)
[ ] Brakes | RELEASE (press PERIOD key)
[ ] VR | ROTATE TO APPROX. 10 DEGREES PITCH UP
[ ] Landing Gear | UP (WHEN POSITIVE CLIMB ESTABLISHED) (press G)
[ ] Airspeed | MAINTAIN V2 UNTIL CLEAR OF OBSTACLES
[ ] Flaps | UP (BLUE LINE, 125 KIAS MINIMUM)
CLIMB |
[ ] Climb Power | 90% N1 TURBINE RPM (OR AS DESIRED) (press F2 or F3 as necessary)
[ ] Propellers | 1600 RPM (OR AS DESIRED) (press CTRL+F2 or CTRL+F3 as necessary)
[ ] Propeller Synchrophaser | ON
[ ] Engine Instruments | MONITOR
[ ] Lights | AS REQUIRED
CRUISE |
[ ] Cruise Power | AS DESIRED (press F2 or F3 as necessary)
[ ] Engine Instruments | MONITOR
DESCENT |
[ ] Altimeter | SET
[ ] Fuel Balance | CHECK
[ ] Power | AS REQUIRED (press F2 or F3 as necessary)
BEFORE LANDING |
[ ] VREF | CONFIRM
[ ] Altimeter | SET
[ ] Flaps | APPROACH (press F7 until APPR)
[ ] Landing Gear | DOWN (press G)
[ ] Lights | AS REQUIRED
[ ] Anti-ice | AS REQUIRED
NORMAL LANDING --When landing is assured--
[ ] Flaps | DOWN (press F7 until DN)
[ ] Airspeed | VREF
[ ] Condition Levers | HIGH IDLE (press CTRL+SHIFT+F3 until fully in)
[ ] Propeller Levers | FULL FORWARD (press CTRL+F3 until fully in)
[ ] Power Levers | IDLE (press F2 until Idle)
--After touchdown-- |
[ ] Power Levers | GROUND FINE (press F2 until fully out)
[ ] Brakes | AS REQUIRED (press PERIOD key)
AFTER LANDING |
[ ] Engine Auto-Ignition | OFF
[ ] Anti-ice | OFF
[ ] Lights | AS REQUIRED
[ ] Transponder | STANDBY (press SHIFT+2 to display radio stack)
[ ] Trim Tabs | SET (with Num Lock off press Num Pad 1 or Num Pad 7 as necessary)
[ ] Flaps | UP (press F6 until UP)
SHUTDOWN AND SECURING |
[ ] Parking Brake | SET (press SHIFT+PERIOD key)
[ ] Avionics Master | OFF
[ ] Lights | OFF
[ ] ITT | STABILIZED AT MINIMUM TEMPERATURE FOR 1 MINUTE
[ ] Condition Levers | FUEL CUTOFF (press CTRL+SHIFT+F2 until fully out)
[ ] Propellers | FEATHER (press CTRL+F2 until fully out)
[ ] Battery and Generator Switches | OFF (below 15% N1)

NOTE: This aircrafts real-world checklists have been modified for use with Flight Simulator.