DEHAVILLAND DHC6 TWIN OTTER
REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Information
articles in the Learning Center. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 10,668 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 170 KIAS
MMO - Maximum Operating Speed Mach | .40 Mach
Turbulent Air Penetration Speed | 130 KIAS
VA - Maneuvering Speed | 105 KIAS
VMC - Minimum Control Speed | 65 KIAS
VX - Two-engine Best Angle-of-Climb | 95 KIAS
VY - Two-engine Best Rate of Climb | 105 KIAS
Best Glide Speed both engines inoperative | 120 KIAS

VFE - Maximum Flaps Extended Speed

Flaps | KIAS
Flaps 10 | 145
Flaps 20 | 135
Flaps 30 | 125
| Flaps 35 | 115

V1 - Takeoff Decision Speed dry runway; Flaps 20
Standard temperature, 5,000' pressure altitude

12,500 lbs | 88 KIAS
<9,500 lbs | 82 KIAS

VR - Rotation Speed dry runway, Flaps 20
Standard temperature, 5,000' pressure altitude

12,500 lbs | 90 KIAS
<9,500 lbs | 85 KIAS

V2 - Takeoff Safety Speed dry runway, Flaps 20
Standard temperature, 5,000' pressure altitude

12,500 lbs | 95 KIAS
<9,500 lbs | 90 KIAS

Airspeed limits (CAS)

Sea level to 4,000 | 165 KIAS
5,000 Feet | 155 KIAS
10,000 Feet | 150 KIAS
15,000 Feet | 145 KIAS
20,000 Feet | 130 KIAS
25,000 Feet | 115 KIAS

VREF - Landing Approach Speed flaps down; gear down

12,500 lbs | 98 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.

Quick Reference - TCAS

+++NOTAMS+++
Check out the Panel_Docs folder...Lot's of Help
Turn on Tool Tips
To raise your seat higher press SHIFT-ENTER
Shift E operates the Pax/Cargo Doors
Shift E +2 will operate the Pilot Doors
If using AUTOSTART.... Check to make sure the Generators are switched to ON in the Overhead Panel
The RED Button on the left / right grips of the VC
Yokes will open the ATC dialog box.
To hear the Exit Door sounds....It has to be quiet in the cockpit Do it before starting engines or after Engine Shutdown
For Best Frame Rates...Keep Windows Closed

    Quick Reference - EYEPOINT KEY COMMANDS

    Move Eyepoint Back

    CTRL+ENTER

    Move Eyepoint Down

    SHIFT+BACKSPACE

    Move Eyepoint Forward

    CTRL+BACKSPACE

    Move Eyepoint Left

    CTRL+SHIFT+BACKSPACE

    Move Eyepoint Right

    CTRL+SHIFT+ENTER

    Move Eyepoint Up

    SHIFT+ENTER

    Reset Eyepoint

    SPACE

Copyright © 2005/2006 - Premier Aircraft Design