DORNIER Do228-212
REFERENCE INFORMATION
For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 14,992 lbs

NOTES:,
(1) To adjust fuel load and passenger/freight load, on the Aircraft menu, click Fuel and Load.
(2) To show and hide yoke in VC use keys Shift-W (FS9) or Ctrl-W (FSX)
(3) This aircraft is un-pressurized and does not normally operate above 10,000 ft

VMO - Maximum Operating Speed | 253 KIAS
MMO - Maximum Operating Speed Mach | .55 Mach
Turbulent Air Penetration Speed | 170 KIAS
VLE - Maximum Gear Operating Speed | 170 KIAS
VLO - Maximum Gear Retraction Speed | 156 KIAS
VA - Maneuvering Speed | 184 KIAS
VMC - Minimum Control Speed | 94 KIAS
VX - Two-engine Best Angle-of-Climb | 125 KIAS
VY - Two-engine Best Rate of Climb | 140 KIAS
Best Glide Speed both engines inoperative | 135 KIAS

Maximum Flap Placard Speeds

Flaps | KIAS
Approach | 202
Full extension | 158

V1 - Takeoff Decision Speed dry runway; flaps up
Standard temperature, 5,000' pressure altitude

15,000 lbs | 108 KIAS
<10,500 lbs | 104 KIAS

VR - Rotation Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

15,000 lbs | 111 KIAS
<10,500 lbs | 104 KIAS

V2 - Takeoff Safety Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

15,000 lbs | 117 KIAS
<10,500 lbs | 98 KIAS

Cruise Climb

Sea level to 10,000 | 170 KIAS

VREF - Landing Approach Speed flaps down; gear down

15,000 lbs | 99 KIAS
14,000 lbs | 95 KIAS
13,000 lbs | 92 KIAS
12,000 lbs | 90 KIAS
11,000 lbs | 90 KIAS
10,000 lbs | 90 KIAS

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.