Jetstream 31 by Premier Aircraft Design
REFERENCE INFORMATION

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VMO - Maximum Operating Speed | 280 KIAS
MMO - Maximum Operating Speed Mach | 0.58 Mach
Turbulent Air Penetration Speed | 200 KIAS
VLE - Maximum Gear Operating Speed | 200 KIAS
VLO - Maximum Gear Retraction Speed | 200 KIAS
VA - Maneuvering Speed | 144 KIAS
VMC - Minimum Control Speed | 110 KIAS

Maximum Flap Placard Speeds

Flaps | KIAS
Approach | 200
Full extension | 160

V1 - Takeoff Decision Speed dry runway; flaps up
Standard temperature, 5,000' pressure altitude

Heavy | 108 KIAS
Light | 95 KIAS

VR - Rotation Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

Heavy | 110 KIAS
< Light | 90 KIAS

V2 - Takeoff Safety Speed dry runway, flaps up
Standard temperature, 5,000' pressure altitude

Heavy | 120 KIAS
< Light | 117 KIAS

Cruise Climb

Sea level to 10,000 | 220 KIAS
10,000 to 15,000 | 210 KIAS

VREF - Landing Approach Speed flaps down; gear down

Heavy | 130 KIAS
Light | 120 KIAS

NOTE 1: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.

NOTE 2: Real world data amended for use in Flight Simulator FS2004 and FSX by Premier Aircraft Design