Hawker Siddeley HS.748 PROCEDURES
For suggested speeds, see the Reference page of the Kneeboard.

Note that most actions can also be performed using the mouse.

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For suggested speeds, see the Reference tab.

For Updates please check ,y website regularly Rick's Paintshop

For support please e mail me or post on the CBFSIM forum
---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------
____________________________________
BEFORE START
[ ] Parking Brake -- SET
(press CTRL+PERIOD key)
____________________________________
ENGINE START
Please note CTRL+E does not work on this aircraft!.

[ ] Fuel Pumps --ON

[ ] Fuel Trim -- SET

[ ] throttle Levers -- CHECK IDLE

[ ] Engine Start Switches -- Select Port/Starb

[ ] Engine Start Switch -- PULL
[ ] Rotating Beacon -- ON

[ ] Altimeter -- SET
[ ] Instruments -- CHECKED
____________________________________
AFTER START
[ ] Engine Start Switches -- FLAMEOUT
[ ] Pitot Heat -- ON
[ ] De-ice -- AS REQUIRED
[ ] Lights -- AS REQUIRED
[ ] Autopilot -- SET and OFF
[ ] Instruments -- CHECKED
[ ] Avionics Switch -- ON
[ ] Avionics -- SET (press SHIFT+2 to display radio stack)
____________________________________
DURING TAXI/BEFORE TAKEOFF
[ ] Parking Brake -- RELEASE
[ ] Thrust Levers-- INCREASE SLIGHTLY TO ROLL (approx 10,900RPM)
[ ] Thrust Levers -- IDLE FOR TAXI
[ ] Flight Controls -- CHECK
[ ] Flaps -- SET FOR TAKEOFF (5)
[ ] Brakes -- SET (press PERIOD key)
____________________________________
CLEARED FOR TAKEOFF
[ ] Engine Start Switches -- GEN
[ ] Flight Director -- ON
[ ] Transponder -- ON
[ ] Lights -- AS REQUIRED
____________________________________
TAKEOFF
[ ] Brakes -- RELEASE
[ ] Thrust Levers -- ADVANCE SMOOTHLY TO 50% (wait for engine stabilization)
[ ] Thrust Levers -- ADVANCE SMOOTHLY TO 100%
[ ] Engine Instruments -- MONITOR
[ ] Airspeed 80 Knots -- CALLOUT "80 KNOTS"
[ ] Airspeed V1 -- CALLOUT "V1"
[ ] Airspeed VR -- CALLOUT "ROTATE"
[ ] Airspeed V2 -- CALLOUT "V2"
[ ] Landing Gear -- UP (WHEN POSITIVE CLIMB ESTABLISHED)
[ ] Airspeed --MAINTAIN V2+20 Knots
[ ] Autopilot -- ENGAGE AT 800 ft AGL
[ ] Flaps-- UP AT 130 Knots
[ ] Throttle Levers -- set 86% 14,200 RPM

____________________________________
CLIMB
[ ] Airspeed -- MAINTAIN 140 - 150 Knots 14,200 RPM (755 TGT)
[ ] Altimeter -- SET TO 29.92 CROSSING 18,000' MSL
____________________________________
CRUISE

[ ] Airspeed -- 190 - 225 Knots
[ ] Thrust Levers-- 14,200 RPM (730 TGT)
[ ] Trim -- AS NECESSARY
____________________________________
DESCENT
[ ] Airspeeds (VREF, VAPP) -- COMPUTED and SET (see the Reference tab of the Kneeboard)
[ ] De-ice -- AS REQUIRED
[ ] Autopilot -- AS DESIRED
[ ] Thrust Levers -- AS DESIRED
[ ] Altimeter -- SET TO LOCAL SETTING CROSSING 18,000' MSL
[ ] Avionics -- SET
[ ] Airspeed -- <250 KIAS BELOW 10,000' MSL
[ ] Landing Lights -- ON BELOW 4,000' MSL
[ ] Approach Procedure -- REVIEW
____________________________________
APPROACH
[ ] Airspeed -- 140 dropping to 115 "over threshold (see Ref for speed)
[ ] Thrust Levers -- Maintain speed
[ ] Flaps -- Approach
[ ] Autopilot -- AS DESIRED
____________________________________
LANDING
[ ] Airspeed -- 100 KIAS
[ ] Thrust Levers -- AS REQUIRED
[ ] Landing Gear -- 160 KIAS DOWN AND LOCKED
[ ] Flaps -- 27.5 Degrees (landing)
____________________________________
LANDING ROLL
[ ] Thrust Levers -- IDLE

[ ] FFP Lamps -- ILLUMINATED
[ ] Brake -- AS NECESSARY
____________________________________
TAXI-IN
[ ] Flap Lever -- UP
[ ] Pitot Heat -- OFF
[ ] Engine Start Switches -- OFF
[ ] Landing Lights -- OFF
[ ] Flight Director -- OFF
[ ] Transponder -- AS REQUIRED
____________________________________
PARKING
[ ] Parking Brake -- SET
(press CTRL+PERIOD)
[ ] Start Levers -- CUT OFF
(press CTRL+SHIFT+F1)
[ ] De-ice -- OFF
[ ] Lights -- OFF
[ ] Transponder -- OFF

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator 2004. To learn about using, printing, and customizing checklists, see Help.

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator.