Hawker Siddeley HS.748 REFERENCE INFORMATION
For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For standard procedures, see the Checklists tab.

For Updates please check ,y website regularly Rick's Paintshop

For support please e mail me or post on the CBFSIM forum

---------------------------------------------------------------------------------------------------------------------------------------

Total Flight Simulator aircraft weight with full fuel
46,500 lbs (MTOW)
NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.
VMO - Maximum Operating Speed (airspeed)
260 KIAS
Turbulent Air Penetration Speed
215 KIAS
VLO - Maximum Gear Operating Speed
160 KIAS
VLE - Maximum Landing Gear Extension Speed
160 KIAS
VLL - Maximum Landing Light Extension Speed
140 KIAS
Maximum Flap (Placard) Speeds
Flaps KIAS
7.5 180
15 180
22.5 140
27.5 120
V1 - Takeoff Decision Speed (dry runway; flaps 5)
Standard temperature, sea level pressure altitude
83 KIAS (46,500 lbs)
80 KIAS (32,000 lbs)
VR - Rotation Speed (dry runway, flaps 5)
Standard temperature, sea level pressure altitude
93 KIAS (46,500 lbs)
92 KIAS (32,000 lbs)
V2 - Takeoff Safety Speed (dry runway, flaps 5)
Standard temperature, sea level pressure altitude
107 KIAS (46,500 lbs)
105 KIAS (32,000 lbs)
VREF - Landing Approach Speed (flaps 22.5, gear down)
115 KIAS (46,500 lbs)
110 KIAS (32,000 lbs)
NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.