CESSNA 414A
REFERENCE INFORMATION
For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel | 6,750 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel and Load.

VA - Maneuvering Speed | 145 KIAS
VLO - Maximum Gear Operating Speed | 175 KIAS
VLE - Maximum Landing Gear Extension Speed | 175 KIAS
Turbulent Air Penetration Speed | 200 KIAS
VNE - Never Exceed Speed | 235 KIAS
VS - Stalling Speed (maximum weight) | 85 KIAS
VSO - Stalling Speed in Landing Configuration | 73 KIAS
VX - Two-engine Best Angle-of-Climb Speed | 115 KIAS
VY - Two-engine Best Rate-of-Climb Speed | 120 KIAS
VXSE - Single-engine Best Angle-of-Climb Speed | 105 KIAS
VYSE - Single-engine Best Rate-of-Climb Speed | 120 KIAS
Minimum Icing Conditions Speed | 180 KIAS
VMCA - Minimum Control Speed | 68 KIAS
Minimum Glide Range Speed | N/A

Maximum Flap Placard Speeds

Flaps degrees | KIAS
15 | 171
30 | 140
45 | 140

NOTE: For explanations of speeds used on this tab, see "V-speeds" in the Learning Center Glossary.